**ITRI Hypervisor Test Case**

|  |  |
| --- | --- |
| **Metadata (Descriptions of the test case)** | |
| **Test case ID** | FT-HFF-BV-0001 |
| **Test case name** | Launch 1 Guest VM |
| **Category** | Hypervisor fundamental functionality |
| **Designer** | Chia Hung Kao |
| **Reviewer** |  |
| **Modified time** | 03/06/2013 |

|  |  |
| --- | --- |
| **Precondition (Conditions that must exist to support the test case)** | |
| **Kernel configuration** | L S - - N B |
| **Host setting** | * CPU: 1 CPU * Memory: 1024 MB RAM * OS: Linux * Network configuration: 192.168.101.2 * Storage configuration: |
| **Guest VM setting** | * CPU: 1 virtual CPU * Memory: 64 MB RAM * OS: Linux * Network configuration: 192.168.20.2 * Storage configuration: NFS |
| **Environment setting** | Host machine is on without any additional process |
| **Steps** | 1. Launch Host machine |

|  |
| --- |
| **Process (Steps to be executed to complete the test)** |
| 1. Login to Host machine 2. Launch Guest VM |

|  |
| --- |
| **Evaluation (Steps to be examined to evaluate the test result)** |
| 1. Guest VM is booted successfully 2. Guest VM can be login |

|  |
| --- |
| **Post process (Steps to be executed to restore the system state)** |
| 1. Shut down Guest VM 2. Shut down Host machine |

|  |
| --- |
| **Related scripts (Scripts used in this test case)** |
|  |